Benjamin Joye, T-00001 Rev A Fluid Sensor Data Acquisition Software

OS: Built for Microsoft Windows 10 Pro, version 10.0.14393

MATLAB: R2007b

Make sure Arduino with Tentacle Shield is connected to COM6.

Atlas Scientific probes required: ORP, EC, Industrial pH

Atlas Scientific EZO circuits (\*\*Serial UART Mode):

- Channel 0: RTD

- Channel 1: pH

- Channel 2: ORP

- Channel 3: EC